11/13/23

Griffin Rzonca

Coding the ESP32 Notes

* Testing with Devkit first
* Plug USB to microUSB connector into UART port
* Test with AD9850 board to ensure proper control
* AD9850 Arduino Library that may work with ESP32: [AD985X/examples/AD9850\_ESP32\_HWSPI/AD9850\_ESP32\_HWSPI.ino at master · RobTillaart/AD985X · GitHub](https://github.com/RobTillaart/AD985X/blob/master/examples/AD9850_ESP32_HWSPI/AD9850_ESP32_HWSPI.ino)